**Coventry University**

**7146CEM: Automotive Software Engineering - Design and Development**

**Coursework: Cruise control system and Motor speed control system**

***Developed by:*** Vignesh Babu Aravamuthan ([adnanv@coventry.ac.uk](mailto:adnanv@coventry.ac.uk))

**Table of content**

[1 Introduction 4](#_Toc89364429)

[2 Software Development Life Cycle 4](#_Toc89364430)

[2.1 Requirement Gathering 4](#_Toc89364431)

[2.1.1 PID controller 4](#_Toc89364432)

[2.1.2 Cruise Control 4](#_Toc89364433)

[2.1.3 Motor Speed 5](#_Toc89364434)

[2.1.4 Code 5](#_Toc89364435)

[2.2 Design 5](#_Toc89364436)

[2.2.1 PID Controller 5](#_Toc89364437)

[2.2.2 PID Tuning Algorithm 7](#_Toc89364438)

[2.2.3 Cruise Control 8](#_Toc89364439)

[2.2.4 Motor Speed 9](#_Toc89364440)

[2.3 Development and Coding 10](#_Toc89364441)

[2.3.1 Cruise Control 10](#_Toc89364442)

[2.3.2 Motor Speed Control 12](#_Toc89364443)

[2.3.3 Code generation 14](#_Toc89364444)

[2.4 Validation 15](#_Toc89364445)

[2.4.1 Validation of Cruise Control Model 15](#_Toc89364446)

[2.4.2 Validation of Motor Speed Model 15](#_Toc89364447)

[3 Advantages of the used SDLC model 15](#_Toc89364448)

[4 GitHub Workflow 16](#_Toc89364449)

[5 Conclusion 16](#_Toc89364450)

[6 References 16](#_Toc89364451)

**Table of figures**

[Figure 1 P Controller Implementation 5](#_Toc89364452)

[Figure 2 I Controller Implementation 6](#_Toc89364453)

[Figure 3 D controller Implementation 6](#_Toc89364454)

[Figure 4 PID Controller Implementation 7](#_Toc89364455)

[Figure 5 Sample Simulation Report 7](#_Toc89364456)

[Figure 6 Cruise Control Schematic 8](#_Toc89364457)

[Figure 7 Motor Speed Schematic 9](#_Toc89364458)

[Figure 8 Cruise Control Block Diagram 10](#_Toc89364459)

[Figure 9 Cruise Plant 10](#_Toc89364460)

[Figure 10 Cruise Control Model 10](#_Toc89364461)

[Figure 11 Cruise Control System Simulation Result 11](#_Toc89364462)

[Figure 12 Cruise Control Plot for Rise Time Analysis 11](#_Toc89364463)

[Figure 13 Cruise Control Plot for Overshoot analysis 12](#_Toc89364464)

[Figure 14 Motor Speed Control Block Diagram 12](#_Toc89364465)

[Figure 15 Motor plant 13](#_Toc89364466)

[Figure 16 Motor Speed Control Model 13](#_Toc89364467)

[Figure 17 Motor Speed Control System Simulation Result 13](#_Toc89364468)

[Figure 18 Motor Speed Control Plot for Rise Time Analysis 14](#_Toc89364469)

[Figure 19 Motor Speed Control Plot for Overshoot Analaysis 14](#_Toc89364470)

[Figure 20 Code Generation Advisor Report 15](#_Toc89364471)

**Table of tables**

[Table 1 Technical Requirements for Cruise Control 5](#_Toc89364484)

[Table 2 Technical Requirements for Motor Speed Control 5](#_Toc89364485)

[Table 3 Cruise Control Model Validation 15](#_Toc89364486)

[Table 4 Motor Speed Model Validation 15](#_Toc89364487)

# Introduction

This document contains information and details regarding the workflow used to create the PID controller, tuning of PID, and generation of code for cruise control and motor speed control project. GitHub is used as a version control system for the project. It is integrated with MATLAB to easily facilitate the GitHub process.

Control systems are needed when the system deals with continuously varying parameters or external disturbances such as load, friction, wind, etc, which will affect the output of the system. To maintain the stable output of the system even in the presence of external disturbances a controller is needed to control those output variations. There are a lot of controlling algorithms available for the control system, we will use only a PID controller for cruise control and motor speed.

# Software Development Life Cycle

This section gives an overall view of the software development process used to develop the cruise control and motor speed system, starting with requirements, design, development, testing, and validation.

## Requirement Gathering

This is the first stage of the V-development cycle that contains a detailed understanding of requirements and expectations for the final product.

### PID controller

#### Technical Requirements

* To design the PID controller using the following equations

Where,

* PID Controller block should contain discrete function blocks.

#### Non-Functional Requirement

* PID controller model should be designed and convert to referenced model.

### Cruise Control

#### Function Requirement

The system should have the following functional requirement:

* Speed of the car should not fluctuate for the external disturbances.

#### Technical Requirement

The system should have the following technical requirements

|  |  |
| --- | --- |
| **S. No.** | **Requirements** |
| 1 | Rise time < 10s |
| 2 | Overshoot < 10% |
| 3 | Stead state error <1% |

Table Technical Requirements for Cruise Control

### Motor Speed

#### Technical Requirement

The system should have the following technical requirements

|  |  |
| --- | --- |
| **S. No.** | **Requirements** |
| 1 | Rise time < 5s |
| 2 | Overshoot < 5% |
| 3 | Stead state error <1% |

Table Technical Requirements for Motor Speed Control

### Code

Developed code for the controller should have the following requirements:

* Code should be optimized for RAM efficiency.
* To develop the code as per ISO26262.
* Code should follow MISRA C Guidelines.

## Design

### PID Controller

#### P Controller Design

P controller is designed by implementing the following equation in Simulink. The following is model is made as a separate subsystem to make it a modular design.




Figure P Controller Implementation

#### I Controller Design

I controller is designed by implementing the following equation in Simulink. The following is model is made as a separate subsystem to make it a modular design.




Figure I Controller Implementation

#### D Controller Design

D controller is designed by implementing the following equation in Simulink. The following is model is made as a separate subsystem to make it a modular design.




Figure D controller Implementation

#### PID Controller Design

P, I, D controllers which are designed as a separate subsystem are integrated by implementing the following equation (refer to Figure 4). The Sampling time of the PID Controller is set to value .

This model is then converted to an atomic subsystem to make it a referenced subsystem. The referenced subsystem is useful in case of multiple definitions of the same PID controller are needed. This referenced subsystem is then used for the Cruise control model and Motor speed control.




Figure PID Controller Implementation

### PID Tuning Algorithm

Script ‘PID\_Turning\_Script.mlx’ is created to obtain , and values to satisfy the requirements. Script uses the trial-and-error method to find the values. The calculation for overshoot, rise time, steady-state error for the output signal is to be implemented in the script to parallelly check whether the requirements are met with corresponding , and values.

The script will also generate a short report (refer to Figure 5) of the output signal and its properties such as rise time, overshoot percentage, output value at simulation stop time, steady-state error percentage for the corresponding , and values.




Figure Sample Simulation Report

### Cruise Control

#### Analysis




Figure Cruise Control Schematic

The vehicle, of mass , is acted on by a control force, . The force represents the force generated at the road/tire interface. For this simplified model we will assume that we can control this force directly and will neglect the dynamics of the powertrain, tires, etc., that go into generating the force. The resistive forces, , due to rolling resistance and wind drag, are assumed to vary linearly with the vehicle velocity, , and act in the direction opposite the vehicle's motion.

#### System equations

With these assumptions, we are left with a first-order mass-damper system. Summing forces in the x-direction and applying Newton's 2nd law, we arrive at the following system equation:

#### System parameters

Parameters of the system are assumed with the following values:

* Mass of the Vehicle () = 1000
* Damping Coefficient () = 50

### Motor Speed

#### Analysis




Figure Motor Speed Schematic

A common actuator in control systems is the DC motor. It directly provides rotary motion and, coupled with wheels or drums and cables can provide translational motion. The electric equivalent circuit of the armature and the free-body diagram of the rotor are shown in the following figure.

The input of the system is the voltage source () applied to the motor's armature, while the output is the rotational speed of the shaft . The rotor and shaft are rigid. The friction torque is proportional to shaft angular velocity.

#### System Equations

The torque generated by a DC motor is proportional to the armature current and the strength of the magnetic field. We will assume that the magnetic field is constant and, therefore, that the motor torque is proportional to only the armature current  by a constant factor  as shown in the equation below. This is referred to as an armature-controlled motor.

The back emf, , is proportional to the angular velocity of the shaft by a constant factor

The motor torque and back emf constants are equal, that is, ; therefore, we will use  to represent both the motor torque constant and the back emf constant. We can derive the following governing equations based on Newton's 2nd law and Kirchhoff's voltage law.

#### System Parameters

Parameters of the system are assumed with the following values:

* Moment of inertia of the rotor () = 0.01
* Motor viscous friction constant () = 0.1
* Electromotive force constant () = 0.01
* Motor torque constant () = 0.01
* Electric resistance () = 1
* Electric inductance () = 0.5

## Development and Coding

### Cruise Control




Figure Cruise Control Block Diagram

The Cruise control system is planned to implement as displayed in Figure 8. Here, Input will be replaced by a ‘Step input’ block. For the PID controller, the referenced subsystem which is created in task 1 is used. The Cruise control plant is modelled (refer to Figure 9) using the mathematical equation defined in 2.2.3.2 above, which is derived from the analysis mentioned in 2.2.3.1 above. With this, the model is developed in Simulink (refer to Figure 10).




Figure Cruise Plant




Figure Cruise Control Model

Parameter and are needed to complete the design, so values are assumed as mentioned in 2.2.3.3 above, and saved the value in MATLAB base workspace. , and values are tuned using the script which is developed. By trial and error method, and values are fixed and varied the parameter once the output signal has reached the desired value then Kp value is set as constant and varied alone, by increasing value it is observed that steady state error was decreasing, when the steady-state error percentage is less than the percentage mentioned in requirements of steady state error values is kept constant, now to remove the overshoot created by increased , is increased to suppress the overshoot. Once the overshoot percentage is less than the percentage mentioned in the requirements of overshoot, calibration is stopped. Now, the PID controller is tuned to meet the requirements. Figure 11, Figure 12, Figure 13 are the simulation result, rise time plot, and overshoot plot respectively is the generated report from the ‘‘PID\_Turning\_Script.mlx’’ script using the Tuned PID Controller.




Figure Cruise Control System Simulation Result




Figure Cruise Control Plot for Rise Time Analysis




Figure Cruise Control Plot for Overshoot analysis

### Motor Speed Control




Figure Motor Speed Control Block Diagram

The Motor speed control system is planned to implement as displayed in Figure 14. Here, Input will be replaced by a ‘Step input’ block. For the PID controller, the referenced subsystem which is created in task 1 is used. The Motor speed control plant is modelled (refer to Figure 15) using the mathematical equation defined in 2.2.4.2 above, which is derived from the analysis mentioned in 2.2.4.1. With this, the model is developed in Simulink (refer to Figure 16).




Figure Motor plant




Figure Motor Speed Control Model

Parameter , , , , , and are needed to complete the design, so values are assumed as mentioned in 2.2.4.3, and saved the value in MATLAB base workspace. , and values are tuned using the same method and the script used in the cruise control development (refer 2.3.1 above). Figure 17, Figure 18, Figure 19 are the simulation result, rise time plot, and overshoot plot respectively, are the generated report from the ‘‘PID\_Turning\_Script.mlx’’ script using the Tuned PID Controller.




Figure Motor Speed Control System Simulation Result




Figure Motor Speed Control Plot for Rise Time Analysis




Figure Motor Speed Control Plot for Overshoot Analaysis

### Code generation

Code is generated using the ‘Embedded coder’ application in Simulink. According to requirement code should design for ‘RAM Efficiency’. All the configuration setting in the code generation is set to meet the requirement. Code generation advisor is used to check whether the generated code is for ‘RAM Efficiency’ (refer to Figure 20).




Figure Code Generation Advisor Report

## Validation

### Validation of Cruise Control Model

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S. No.** | **Requirements** | **Input** | **Requirement**  **Criteria** | **Result** | **Status** |
| 1 | Rise time | 0-1000  (Step input) | Less than  10 seconds | 0.4 seconds | Accepted |
| 2 | Overshoot | 0-1000  (Step input) | Less than 10% | 0.5% | Accepted |
| 3 | Stead state error | 0-1000  (Step input) | Less than  1% | 0% | Accepted |

Table Cruise Control Model Validation

### Validation of Motor Speed Model

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S. No.** | **Requirements** | **Input** | **Requirement**  **Criteria** | **Result** | **Status** |
| 1 | Rise time < 5s | 0-100  (Step input) | Less than  5 seconds | 0.1 Seconds | Accepted |
| 2 | Overshoot < 5% | 0-100  (Step input) | Less than  5 % | 0 % | Accepted |
| 3 | Stead state error <1% | 0-100  (Step input) | Less than  1 % | 0 % | Accepted |

Table Motor Speed Model Validation

# Advantages of the used SDLC model

* The V-shaped model should be used for small to medium-sized projects where requirements are clearly defined and fixed since the requirements are very clear for cruise and motor speed control systems V-Shaped model is used.
* Proactive defect tracking – that is defects are found at an early stage.
* Simple and easy to use

# GitHub Workflow

GitHub is integrated with MATLAB, and all the versioning process is done within MATLAB itself. The link for the repository is as follows:

<https://github.com/vigneshbabu0717/coursework_7146CEM_vigneshbabu_11911348.git>

# Conclusion

Cruise control and Motor speed control system is developed with V-development cycle as SDLC. Requirements are gathered from the task given and using the requirements, a design for both systems is created. After the design, actual development is done in Simulink. Finally, validated the output of the developed system with requirements to check whether all the requirement criteria are satisfied or not.

# References

*Control Tutorials for MATLAB & Simulink*. (n.d.). Retrieved from https://ctms.engin.umich.edu/CTMS/index.php?example=CruiseControl&section=SystemModeling

*Control Tutorials for MATLAB & Simulink*. (n.d.). Retrieved from https://ctms.engin.umich.edu/CTMS/index.php?example=MotorSpeed&section=SystemModeling